*HEADING
FESA recognized no-op heading
*PREPRINT, ECHO=NO, MODEL=NO, HISTORY=NO, CONTACT=NO
*NODE
1, 0.0, 0.0, 0.0
2, 1.0, 0.0, 0.0
*ELEMENT, TYPE=B31, ELSET=Beam
1, 1, 2
*NSET, NSET=Fixed
1
*ELSET, ELSET=Beam
1
*MATERIAL, NAME=Steel
*ELASTIC
200.0, 0.25
*BEAM GENERAL SECTION, SECTION=GENERAL, ELSET=Beam, MATERIAL=Steel
1.0, 1.0, 0.0, 1.0, 1.0
0.0, 1.0, 0.0
*STEP
*STATIC
*BOUNDARY
Fixed, 1, 6
*CLOAD
2, 2, -1.0
*RESTART, WRITE, FREQUENCY=0
*OUTPUT, FIELD, VARIABLE=PRESELECT
*OUTPUT, HISTORY, VARIABLE=PRESELECT
*END STEP
